This Board is with 5 steppers.  
I need X and Y step dir signals only without driver.  
Rest 6 axis with driver socket replaceble with TMC2209 or DRV8825.  
Keep all functions intact.  
Have to replace MCU and use STM32H723